<HTML>
<HEAD>
  <TITLE>APP_GIS1_de.htm</TITLE>
  <META HTTP-EQUIV="CONTENT-TYPE" CONTENT="text/html; charset=windows-1250">
  <meta name="description" content="GIS Applikation Spezifikation">
  <meta name="keywords" content="GIS CivilEngineering">
  <meta name="date" content="2011-01-23T09:52:24+0100">
  <meta name="author" content="fwork">
  <META NAME="CHANGEDBY" CONTENT="David Young">
  <META NAME="CHANGED" CONTENT="20090906;17143200">
  <META NAME="CREATED" CONTENT="200703250">
  <style>body{ font: 10pt Verdana,sans-serif;}</style>
</HEAD>
<BODY LANG="en-US">
<PRE>
<h2>Documention Application GIS1</h2>
Version 2.0 - 2011-01-17

<b> program call: </b>
    Start the user application "APP_GIS1"
      - Select from the list of add-on applications or
      - if application was active before: start with Ctrl-P


<b> termination of the application: </b>
  Exit button.
  It will pass all data to the CAD model.



<A HREF='#fAux'>toolbox</A>
<A HREF='#edit'>modify points, surfaces</A>
<A HREF='#proj'>project objects to surface</A>
<A HREF='#edge'>define boundaries, breaklines</A>
<A HREF='#Todo'>ToDo</A>



____________________________________________________________________________
<p><a name="fAux"></a></p>

<h3>Import points from ascii-file:</h3>
  One point per Line.
  The first word that contains a dot (Decimalpoint, &quot;.&quot;) is used
  for the X-Coordinate; the following two words are used for the
  Y- and Z-Coordinates.
  Additional textinfos (Words before or after the Coordinates)
  are not used at the moment.

  Example:
    import file &quot;sample_gispoints1.txt&quot;,
      (&quot;ImportPoints&quot;; Filtertext &quot;gis&quot;)
    rescale model with button &quot;Scal.All&quot;
    &quot;create Mesh&quot; to create/display the TIN
    &quot;Exit&quot; to transfer date to model
    File/save Model as/VRML2 to create a WRL file.


<h3>Export points into ASCII file:</h3>
  Menu item "File / Export points"
  The Coordinates of the Points of the active Point-surface are
  written out into a file.
  At the moment no additional textinfos are written.


<h3>Display the coordinates of all points of the active GIS Area:</h3>
  Menu item "Tools / dump all points"
  HTML file {tempDir}/tmp.htm is generated and displayed.


<h3>Display a list of all edges of the active GIS Area:</h3>
  Menu item "Tools / dump all edge lines"
  HTML file {tempDir}/tmp.htm is generated and displayed.


<h3>print the current view:</h3>
  Menu item "Tools / print"


____________________________________________________________________________
<p><a name="edit"></a></p>
<h2>"edit" - modify points, surfaces</h2>

<h3> create new GIS-points: </h3>
  - indicate position with the left mouse button or
  - Select an existing CAD-point or
  - Enter the coordinates into the fields X, Y, Z; button "AddPt.".


<h3> move GIS-point: </h3>
  The active (last selected) point is moved;
  using the coordinates of the fields X, Y, Z;
  Button "Mod.Pt.".


<h3> Move all GIS-points: </h3>
  Menu item "Tools / move all points"
  Enter the offset.


<h3> Delete GIS-points: </h3>
  select them individually or as a group, "Delete" button.


<h3> Delete subsequent points: </h3>
  Menu item "Tools / delete range of points"
  Type the Point numbers of the first and last point.


<h3> Delete GIS-edge: </h3>
  Select edge, button "Delete".


<h3> Delete network: </h3>
  Select network (A), button "Delete".


<h3> Recalculate network: </h3>
  Button "create mesh".


<h3> network boundary clean: </h3>
  Menu item "Tools / remove outer zone"
  Automatic removal of triangles with too long sides.


<h3> Changing the active surface: </h3>
  Select from the list of loaded areas (far left).
  Only the active area can be modified.


<h3> Create new surface: </h3>
  If no GIS area is included in the model, the start of the function
  automatically generates a new (empty) GIS area.
  With this feature, another new GIS area is generated:
  Menu item "Tools / create new surface"


<h3> Delete active area and all of their points: </h3>
  Menu item "Tools / delete active mesh and all points"
  The currently active GIS area and all of its points will be deleted.




____________________________________________________________________________
<p><a name="proj"></a></p>
<h2>"prj -> Mesh" - project objects to surface</h2>

<h3> project point onto the net and generate GIS-point: </h3>
  - indicate position (left mousebutton) or
  - select CAD-point


<h3> project curves on the Net: </h3>
  select CAD-curve, another CAD-curve is created.
  Attention: the curve must be located within the Network!   (TODO)



____________________________________________________________________________
<p><a name="edge"></a></p>
<h2>"create Edge" - define boundaries, breaklines</h2>
create outer Network boundaries outside,
create inner Network boundaries (holes, void areas),
create breaklines (edges).

First define the edgeline, then select the edgetype.

  define consecutive edges by -
  - select GIS points or
  - select curve. The required GIS-points are generated.

  CAUTION:
  - Edge lines may not cross;
  - breaklines may not cross outer and inner boundaries. (TODO)



____________________________________________________________________________


If necessary adjust Model Size:
  (Standards / Tolerances / model size = 15000, Modify, Exit).



<b> Program Files: </b>
  APP_GIS1 is a supplementary program to gCAD3D.
  The source code file is ../GIS1/APP_GIS1.c
  The APP_GIS1 license program is GPL.

  Please report problems / corrections to
  franz.reiter @ cadcam.co.at


____________________________________________________________________________
<p><a name="Todo"></a></p>
<h2> TODO: </h2>
<b> LandXML import: </b>
  - Import breaklines
  - Import Void-area (hole inside Borders)

<b> LandXM create export </b>


<b> undo / restore for deleted objects </b>



</PRE>
</HTML>
