##

    First steps - documentation to gCAD3D - NC

    -------------------------------------------------------------------------

    Numerical control programs must be made at present in the mode MAN;
     see in addition Help / getting started  MAN.

     The numerical control words (RP, (STOP FED COOL INSERT.)) must be entered
     at present with the keyboard.

     With Alt-F "FROM", with Alt-W "WORK" is produced.
     Associated geometrical objects (points, outlines) can be selected.
     Conclusion with RETURN key or right mouse button.
     At each time one can re-establish each programstate with the cursor key up/down.

     You have to provide the partContour, starting points and workingContours
       with CAD or MAN.

    # Example:
    # start points:
    P20=P(100 100)
    P21=P(200 100)
    P22=P(50,50)
    P23=P(85 140 0)
    P24=P(120 140 0)
    P25=P(250 95 0)
    P26=P(260 100)
    P27=P(225 150)
    # partContour
    S20=REC P22 D(260 0 0) D(0 128 0)
    # workingContours
    S21=CCV  P23 P(92 140 0) P(95 150 0) P(100 150 0) P(103 140 0) P(110 140 0)
    S22=CCV  P24 P(140 140 0) P(130 160 0) P24

    # definition lower level
    ZSUR1 0
    # definition upper level
    ZSUR2 50
    # start without Tool
    TL 0
    # definition of the starting point;
    # represented by a triangle
    FROM P22
    # rapid path:
    # is dash-dotted represented, relative with "RPR" RP P20
    RP P20
    # toolchange instruction
    TL 1
    # work contour (CCV, "S") at the momentary position:
    WORK CUT S21
    WORK CUT S21
    # linear treatment (representation as surface):
    # relative linear treatment: "WORK PR  "
    WORK P21
    TL 0
    RPR 25 0
    TL 1
    # work circular:
    # radius startingdirection circular-angle driving-out-distance
    WORK CUT_CIR 12 0 360 0
    TL 0
    RP  P27
    TL 1
    # circular pocket cycle:   outer-radius inner-radius
    WORK POCK_CIR 12 5
    TL 0
    # starting point pocket (within outline) RP P26 tl 1
    RP P26
    TL 1
    # definition edge-distance cut-distance
    POCKET 1 3
    # pocket cycle: Outline, outline-starting point
    WORK POCK S22 P25
    # finish contour
    WORK P25
    WORK CUT S22
    TL 0
    RP P22
    #

    -------------------------------------------------------------------------

     All further information in the documentation.