LANG__=English

MM0=display functions:\
\move:=  Shift + drag mouse (do not push mousebuttons)\
\rotate:=Ctrl + drag mouse\
\zoom:=  Shift + Ctrl + drag mouse

MMclear=clear modelspace
MMmock=only OBJ-models; ON: import model; OFF: load model, modify and export not possible.
MMsave=save native (.gcad-format)
MMcomp=compress native Models (.gcad) with gzip (.gcaz)
MMfDel=delete File
MMfRen=rename File
MMfCpy=copy File
MMfPrt=print / plot
MMexit=exit program
MMsma=activate mainmodel or other submodel
MMsmcp=move mainmodel into submodel
MMsmcr=create new submodel
MMsmsf=save the active submodel into file
MMsmlf=load modelfile as submodel
MMsmre=rename the active submodel
MMsmde=delete the active submodel
MMsmmp=modify the Position of a subModel

MMopBnd=display Edgelines; ON / OFF
MMopDll=compile and link plugin-programs before starting; ON / OFF
MMopInt=activate interactions; ON / OFF
MMopTb1=display MainToolBar (above grafic); ON / OFF
MMopTb2=display MessageToolBar (below grafic); ON / OFF
MMopBrw=display Objectbrowser (left of grafic); ON / OFF

MMdsps=save active view
MMdspsr=restore stored view and save active view
MMdspr=restore stored view

MMdspon=display objectnames and (working-)-directions
MMdspdir=display direction of curves
MMdsppt=display points (P) on / off (only in VWR)
MMdsppl=display planes (R) on / off (only in VWR)
MMdspso=display Solids (Sphere/Cone/Torus/Cube) shaded or wireframe

MMstTol=define Modelsize and Tolerances
MMstTxl=define Textsize for Notes and Dimensions
MMstCol=define Default-Modelcolor
MMstLty=define Linetypes (Color-Lintyp-LineThick) for Lines/Circs/Curves
MMstDir=define Modeldirectories
MMstBrw=define Browser for help / documentation
MMstEdi=define Editor

MMmdMsi=set size and tolerances of model
MMmdMdp=modify the Position of a subModel
MMmdCvC=change curves into circles
MMmdLty=change Linetyp (Colour, Linetyp, LineThick) of Lines/Circs/Curves
MMmdSst=change SurfaceStyle to shaded or symbolic (wireframe)
MMmdSco=change Color of Surface to active Color)
MMmdpsr=make Surface transparent
MMmdStx=make textured surface
MMmdOnm=display a list of objects
MMmdDel=delete objects
MMmdEdi=modify active inputfield with systemEditor / F3
MMmdCln=remove all deleted Lines permanent / F4
MMmdDlo=undo (delete last operation; Ctrl-Z)
MMmdRlo=redo (restore last operation; Ctrl-Y)

MMinVpt=give ViewportParameters (into open Interaction)
MMinTxt=MAN: paste textBuffer after delete or ctrl X

MMsePcp=give Coordinates of cursor on construction-plane at next selection
MMsePop=give parametric point of cursor on selected object at next selection
MMseLoO=get line from a segment of a polygon or countour at next selection

MMgrAdd=add obj to group; remove from Group, if already selected
MMgrSav=save all objects of Group into File (native)
MMcaMod=Modify standardparts
MMcaCre=Create new Catalog of standardparts
MMcaDel=Delete Catalog of standardparts
MMapSta=Load and start application (script)
MMapEdi=edit the active  application
MMapCre=Create new Application
MMapDel=Delete Application

MMbtgo=regenerate all objects up to the active object
MMbtstp=recreate active object
MMbtend=regenerate all objects
MMenZva=set the Z-value of the active viewplane
MMcbRot=define rotation-center for interactive rotation
MMcbHid=do not display selected objects
MMcbVie=redisplay hidden objects
MMcb3dv=inhibit 3D-Rotation; ON / OFF
MMcbSha=display of surfaces shaded or wireframe

MMbtTop=topview (X-Y)
MMbtFro=frontview (X-Z)
MMbtSid=sideview (Y-Z)
MMbtAxo=axonometric view
MMbtSca=compute scale and viewcenter automatic
MMbtScf=display a space of ~ 6000 x 6000 x 6000 mm
MMbtScg=scale to active group
MMbtVwpt=save / restore current viewport (Ctr-V, Ctrl-CursorRight)
MMrbRel=display cursorposition on the active constructionplane
MMrbAbs=display cursorposition on the active constructionplane as absolute coordinates

MMrbVwr=Viewer
MMrbNCw=not active
MMrbCad=interactive CAD-Object-Editor
MMcbSN=search object, add/modify object-name
MMrbMan=manual mode (create/modify objects with texteditor)
MMcbMD=Search / Modify / Delete obj  (Ctrl+leftMouseButt or Ctrl-F)
MMundo=undo (delete last operation; Ctrl-Z)
MMredo=redo (restore last operation; Ctrl-Y)

CADPT=Points
CADLN=Lines
CADCI=Circles
CADPLN=Planes
CADVC=Vectors
CADVAR=Variables
CADCV=Curves (Ellipse, Polygon, Spline, Clothoid, Contour (composite curve))
CADSUR=Surfaces
CADSOL=Bodies
CADDIM=Text, Dimensions
CADMDL=Submodels
CADTR=Transformations
CADCUT=Trim, intersect, move, rotate, project, mirror
CADINT=Interactions, joints
CADANA=Analyze
CADCP=Constructionplane

RotCen=define new rotation-center:\
\-=select (existing) vertex or -\
\-=rotate display (Ctrl-drag_mouse) and select red star
ViewOn=display hidden objects; select objects to display
HideOn=select objects to hide
VWR_On=VWR: zoom/pan with mouse and shift/ctrl-key; select obj to analyze
CAD_On=CAD: select Function / select object with right mouseb.
MAN_On=MAN: new point: Alt-P; newline: right_mousebutton; ..
MD_On=select object / key ObjID Enter / Exit: Ctrl right mouseb.

CADname=Objektname / info (search it with "Search/Name")
CADhelpCAD=display a Help-text how to use CAD in a html-browserwindow
CADhelpFunc=display a Help-text for active Function in a html-browserwindow
CADhelpInput=display a Help-text for active inputfield in html-browserwindow
CADexit=cancel function. Does not save active object. Edit-mode: Cancel twice, right mousebutton  - edit.
CADclear=clear active CAD-inputfield
CADsave=save active obj., goto next obj. Right mousebutton, Enterkey.

PT_cartes__offset=point; select or key; [offsetvalues for X/Y/Z]
PT_polar=polar, relativ; Basepoint, Rotationangle (Z-Axis), [Tiltangle (X-Y-plane),] Distance
PT_translate=move point; Basepoint, Direction, [Distance,] [NormalDistance]
PT_rotate=rotate point; Centerpoint, Startposition, Angle [Axis]
PT_endpoints_center_focus___=characteristic points (center-, start-, end-; focus for ellipses, cornerpoints for polygons, splines)
PT_Mid_Cornerpoint_PT_PT__VC_=midpoint or cornerpoint of 2 points
PT_parametric_on_LN_CIR_CRV_SUR=Point from parameter(s) on Line/Circle/Curve/Surface

LN_PT__PT=Line between 2 points
LN_parallel=Line parallel tu line/vector
LN_PT_Direct__Length_Rot_Angle_TiltAngle_=Line by point and direction, [length,] [Rot.Angle (Z-Axis),] [TiltAngle (X-Y-plane)]
LN_LN_Dist____________parall_=Line parallel to line; distance, position (1-4).
LN_LN_LN__Rot_Angle_TiltAngle___mid_=Line = midline; [rotate in intersectionpoint: Rotationangle (Z-Axis), [Tiltangle (X-Y-plane)]
LN_tangent_to_line_circ_curve=line tangential to 2 objects (point/direction/circle/ellipse/bspline)

CIR_Cen_Radius__Z_Axis_=Circle from center, radius [Axis]
CIR_Cen_Tang=Circle from center, tangential to point/line/circle
CIR_Tang_Tang_Radius=Circle tangential to two elements, with fixed radius
CIR_Tang_Tang_Tang=Circle tangential to 3 elements
ARC_Cen_Ang1_Ang2_Radius=Circ.Arc by center, start angle, end angle and radius
ARC_Cen_PT_Angle=Circ.Arc by center, start point and opening angle
ARC_PT_PT_Radius=Circ.Arc by start point, end point and radius
ARC_PT_Tang_Radius__Angle_=Circ.Arc by start point, start direction and radius [opening angle]
ARC_PT_PT_Cen=Circ.Arc by start point, end point, center
ARC_PT_PT_PT=Circ.Arc by 3 points on the arc

PLN_Z_Axis__X_Axis_=Plane from origin, Z-axis (normalvector), [x-axis-vector or point on x-axis]
PLN_X_Axis__Y_Axis_=Plane from origin, X-axisvector, [y-axis-vector or point on y-axis]
PLN_PT_Plane_Offset_Angle=Plane with new origin and/or rotated around Z-axis

VEC_cartes__polar=Vector from line or vector or cartes. [length] [REV (turn)]
VEC_polar_______Angles_Length_=Vector from Rot.Angle (Z-Axis), [TiltAngle (X-Y-plane)] [length] [REV (turn)]
VEC_from_objects=Vector = tangent to curve (Circ/Ellipse/B-spline/Clothoid) from point on curve

V_Variable___Value=variable from value
V_X_Y_Z_part_PT_VC=variable from X- Y- or Z-part of a point or vector.
V_PT_PT_Dist__Direction_=variable = length between 2 points [direction -vector]
V_LN___Length=variable = length of a line
V_PT___LN_Perp_Dist_=variable = normal distance of a point to a linear object
V_CIR__Radius=variable = radius of a circle

S_Ellipse_Center_AxisEndPoint_Point=Ellipse from center, end point main axis, point on ellipse
S_Ellipse_Center_Axes__EndPoints_=ellipse (limited) from center, vector main axis, vector secondary axis, start point, end point
S_Polygon___Points___=Polygon from points
S_Polygon___Rectangle=Parallelogram from cornerpoint and 2 vectors
S_BSpline___Points___=B-Spline from points; [CTRL (controlpoints/through-points)]
S_BSpline___Polygon___=B-Spline from polygon; [CTRL (controlpoints/through-points)]
S_BSpline___convert___join_obj_s=B-Spline = join (connect) lines/circs/b-splines
S_Clotoid=Clothoid from StartPoint, StartVector, Angle, StartRadius, EndRadius [Z-Axis]
S_connection_lines___Points___=connecting lines between points
S_Contour_CCV_____PT_LN_CIR_CRV=Contour (composite curve - CCV) from startpoint, curves, endpoint. Automatic intersecting and trimming.

A_Planar_Surf__trim_punch_=Planar surface from boundary (circle/polygon/contour) [islands (circle/polygon/contour)]
A_Spheric_Surf__Axis_Rad__=Spherical surface from axis, radius [angle-x1,x2] [angle-y1,y2]
A_Cylinder_Surf__Axis_Rad__= Cylindrcal surface from axis, radius [angle-x1,x2] [angle-y1,y2]
A_Revolved_Surf__Axis_Contour_=Revolved surface from axis, contourline (line/circle/b-spline), [startangle] [endangle] height1 (parameter or point), height2 (parameter or point)
A_Extrusion_Surf__Contour_Vec_= Ruled surface from linear element (line/circle/b-spline) and vector
A_Sweep_Surf__Contour_Path_=surface from path (spine) and contour (eg pipe)
A_Loft_Surf__Curves_across_=Freeform surface from vertical sectioncurves (line/circle/b-spline)
A_Loft_Surf__Curves_along_across_=Freeform surface from horizontal and vertical sectioncurves (line/circle/b-spline)
A_supported_trimmed_punched=Trimmed surface from supporting surface, boundarycurve [islands ...] 
A_Hatch___Schraffur=Hatched surface from boundarycurve, linedistance, angle.

B_Conus_PT_PT_R_R=Cone from 2 points and 2 radii
B_Conus_Circ_height_radius=Cone from from circle, height and radius
B_Torus_Axis_R_R=Torus from central axis, outer radius and inner radius
B_Torus_Axis_CI=Torus from axis and circle
B_Sphere_Center_radius=Sphere from center, radius/point/circle
B_Prism_Base_Thick_Point_Cone_=Prism from base area (circle/polygon/contour) and thickness/Point
B_Prism_Base_Vec=Prism from base area (circle/polygon/contour) and vector

N_DIM__hor_vert_parall_=Linear dimension 2D
N_DIM3_X_Y_Z_parl=Linear dimension 3D
N_DIM__Angle=Angle dimension 2D
N_DIM__Dmr=Diameter dimension 2D
N_DIM__Radius=Radius dimension 2D
N_PointPos_LN=3D-coordinates of a point with leaderline
N_Text=3D-Text with variable size, direction and special characters.
N_Text_LN=Text with 1 or 2 2D-leaderlines, [with arrowhead]
N_Text_LN_Circle=Text with a circle and 2D-leaderline
N_TextTag_LN=2D-Textblock [with leaderline]
N_Symbol=Symbol (0-5, star/triangle/circle/rectangle/arrow1/arrow2)
N_Image_Pos_Filename=Image (normal to the viewer, scale fixed or dynamic)

M_internal_Model=internal submodel; position, scale [orientation]
M_external_Model=external submodel; position, scale [orientation]
M_CatalogPart=Standardpart; position, scale [orientation]

TRafo_transl=Translation from direction [length]
TRafo_rot=Rotation from axis, angle

CUT__trim__obj=Trim linear elements (line/curve) with one or two cutting elements
INT__intersect__obj=Intersectionpoint or -curve from intersection of 2 elements
TRAnslate_obj__VC_=move element along vector [length]
TRAnslate_obj__PLN_=Move an object to a different reference system (plane) [TRA - invert transformation]
TRAnsform_obj__Tra_=Objekt verschieben (Verschiebung) oder drehen (Verdrehung)
REV__reverse__curve=reverse curve
Project_obj__Prj_=Project element onto a surface
Mirror_about_line=Mirror: reflect objects across line
Mirror_about_plane=Mirror: reflect objects across plane
ISOparametric_Curve_from_Surf=extract curve from surface (from paramtere(s)); [CX (across; Default = along)]

Interact_connect=connect object with interaction
Joint_export=export object (point or text)
Joint_import=import object (point or text) from submodel

Analyze_Point_Posi_=Displays the point coordinates
Analyze_Obj_=Display object type and coordinates
Analyze_Dist__PT_PT=Measures the distance between 2 points
Analyze_Dist__PT_Obj=Measures the normal distance between point - object
Analyze_Vertex=Displays the coordinates of a vertex point (a displayed 3D-point)

ActiveConstrPlane=activate constructionplane from plane
Reset_ConstrPlane=reset constructionplane (activate standard-coordinate-system)

Typ_Val=Key Val / PgUp / PgDwn / Sel LN (Len.) / Sel Cir (Radius)
Typ_PT=Sel PT (on obj) / Indicate PT / key coords
Typ_LN=Sel LN
Typ_AC=Sel CIR
Typ_VC=Vector: Key PgUp/Dwn / D[I]X/Y/Z / dx dy [dz] ANG(ax) [ANG(az)]; Sel LN/Cir/Elli/Surf/PLN/PT+PT / "REV" (turn)
Typ_CV=Sel CRV
Typ_CVCCV=Sel CCV
Typ_CVPOL=Sel Polygon
Typ_XVal=Key X-Val; Sel PT
Typ_YVal=Key Y-Val; Sel PT
Typ_ZVal=Key Z-Val; Sel PT
Typ_Angle=Angle: Key Val(Deg.); Sel LN / PT-PT; Key PgUp/Dwn
Typ_PLN=Sel PLN; Key PgDwn (ConstrPln)
Typ_SOL=Sel Conus/Torus
Typ_goPrim=Sel PT/LN/CIR
Typ_lFig=Sel LN/Cir/CRV
Typ_goGeom=Sel Object
Typ_goGeo1=Sel LN/Cir/CRV/PLN
Typ_goGeo2=Sel Circ or Ellipse
Typ_goGeo3=Sel PT/LN/Cir/CRV, CW/CCW
Typ_goGeo4=Sel VC / LN / PLN
Typ_goGeo5=Sel CIR/ELL/CCV
Typ_goGeo6=Key Angle (degree); Sel Vec/LN for direction; ReversButton
Typ_goGeo7=Key Val(Angle-Degree); Sel PT
Typ_goGeo8=Key Val; Sel PT
Typ_goAxis=Sel LN / Cir / PLN / PT+PT / PT+LN / PT+VC (PgUp) / PT+PLN
Typ_goRadius=Key Radius; Sel PT / Cir
Typ_goGeoSUSU=Sel Conus Torus RuledSurf RevolvedSurf B-Spl-Surf
Typ_Tra=Key PgUp/Dwn (select Transformation)
Typ_modAux=Key PgUp/Dwn
Typ_mod1=Key PgUp/Dwn (selects alternate versions)
Typ_modCWCCW=ReversButton; PgUp/Dwn; Key "CW" (clockwise)
Typ_modCTRL=Key PgUp / PgDwn  ("CTRL" = Controlpoints)
Typ_modREV=Key PgUp / PgDwn  ("REV" = reverse)
Typ_modCX=ey PgUp / PgDwn  ("CX" = across)
Typ_modUnlim=Unlimited; PgUp or PgDwn or key "UNL" or "UNL1" or "UNL2"
Typ_modRepl=replace obj default = copy Key PgUp/Dwn or "REPL"
Typ_Txt=enter text / key PgUp / PgDwn
Typ_String=Key Text / Modify-Edit
TYP_FilNam=Key Filename / middle Mousebutt.(F5=FileList) / sel.Model
Typ_CtlgPart=Key  Catalog/Part / middle Mousebutt.(F5=FileList) / sel.CatalogPart
Typ_Model=Key Modelname / sel.Model
Typ_SubModel=Key Modelname / middle Mousebutt.(F5) / sel.Model
Typ_Str_Dir1=Key X / Y / Z / P / PgUp/Dwn
Typ_Val_symTyp=Key 0 (Star) 1 (Tria.) 2 (Circ) 3 (Rec.)
Typ_Joint=key joint / select joint
Typ_apDat=Key application-specific data
Typ_Group=Sel obj's to add to group; exit with Tab-key

XAesc=user abort (esc-key)
VC0=no Vektors defined ..
VR0=no Variables defined ..

FILT02=Pointfilter Vertex
FILT03=give position of cursor on selected obj ..
FILT04=select or keyIn obj to dump ..
FILT05=add following selections/keyIn to group, end group with Tab-Key
FILT06=select Line|Circ|Curve to modify ..
FILT07=select surf to modify ..
FILT13=select surf to remove texture
FILT14=select surf to apply texture
FILT15=select surf to load texture
FILT16=modify position: select subModel
FILT18=get point as parametric-point of next selected obj ..
FILT19=get line from a segment of a polygon or countour at next selection ..

DIR_NEW=select new directory (no symbol exists)
DIR_SYM=select symbolic directory (from existing symbol)

PEDnopt=Object does not have moveable points ..
PEDnrpt=Object has  {0}  moveable points ..
PEDsav=save modifications (ri.Mousebutt.)
PEDcanc=cancel modifications (Esc-key)
PEDlink=break link to obj {0}  ?
PEDmod1=give plane or vector / sel. point (yellow square, Sym-#) / Delete / Insert / Exit: ri.Mousebutt.
PEDmod2=give plane or vector / sel. point (yellow square, Sym-#) / Exit: ri.Mousebutt.
PEDmod3=Save (ri.Mousebutt.) or Cancel (Esc-key)
PEDmov=move point (move mouse); -  end with right mousebutton ..
PEDdel=Delete point: select point (yellow square, Sym-#) to delete / Modify / Exit: ri.Mousebutt.
PEDins=Insert point: select position on curve - where to insert point / Delete / Modify / Exit: ri.Mousebutt.
PEDine=***ERROR: select insertposition on active curve ..
PEDerrSel=*** ERROR: cannot use selected object ..
PEDe1=*** ERROR: PointEditor is active ..
PEDe2=*** ERROR: cannot analyze Plane/Vector
PEDe3=*** ERROR: cannot insert point ..

TED_no=no Texture is active
TED_ldf=load image
TED_ldf=load texture from imagefile
TED_ldn=reload
TED_ldn=reload imagefile
TED_rem=remove
TED_miy=mirror vertical
TED_mix=mirror horizontal
TED_sz1=fit into
TED_sz2=fixed size
TED_can=reset and exit (Esc-key)
TED_end=save and exit (Return-key)

UIWTms=Modelsize. All following values will be recomputed.
UIWTcv=max. deviation for curves (tolerance for approximation curve -> polygon)
UIWTdi=max. display-deviation for circles, curves
UIWTsm=set only for the active model or apply to all subModels
UIWTmo=activate the modelsize / tolerance from above
UIWTre=reset all values to default (modelsize 500)

MMcbMea=measure between 2 points
Meas_in=Measure: select 2 points; end with right mousebutton.
LST_err1=list overflow; enter text for filter
SEL_fnam=select or key filename
SEL_sDir=Give symbolic pathname for dir.  {0}
SEL_ko=Object  {0}  cannot be used ..
OVER_fil=overwrite file  {0}
OVER_mdl=overwrite submodel  {0}
NOEX_fil=file  {0}  does not exist
NOEX_mdl=subModel  {0}  does not exist
NOEX_dir=directory  {0}  does not exist
ModColIn=define new Color, then select surface ..
ModTraIn=define 50% or 80%, then select surface or body ..
ModSstIn=define new surfacestyle, then select surface or body ..
ModLtyIn=define new linetype, then select line or curve ..
CADinit=Save: OK or right mousebtton or Enter-key; Abort: Cancel or Esc-key.

SN_New=create new group (from complete model)
SN_Add=add to active group (from complete model)
SN_Rem=remove from active group
SN_TxtNot=search all objects [NOT] containing infotext
SN_DepNot=search all objects [NOT] depending from object "depends"

ERRCAD0=ERROR: function CAD must be active ..
pluginErr0=rebuild not possible - compiler or linker not found.
pluginErr1=Error in plugin  {0} ; aborted.
FileOp=opening file  {0}
SAVusm=Save unused submodel  {0}  ?

ED1CW=last input clockwise
ED1CCW=last input counterclockwise
ED1MOD+=select next solution-variant
ED1MOD-=select previous solution-variant
ED1<<<=one input back (before inserting)
ED1>>>=one input forward (after inserting)

EOF
