##

##

##

##

##

    See operating CAD

    CAD functions for planes and axis systems:

    Planes and axis systems use the shortcut letter R.

    Pre-defined planes are:
    Vordefinierte Ebenen sind:

    RZ   XY (Z=0)  Plane-X = Refsys-X
                   Plane-Y = Refsys-Y
                  (Plane-Z = Refsys-Z)

    RY   XZ (Y=0)  Plane-X = Refsys-IX
                   Plane-Y = Refsys-Z
                  (Plane-Z = Refsys-Y)

    RX   YZ (X=0)  Plane-X = Refsys-Y
                   Plane-Y = Refsys-Z
                  (Plane-Z = Refsys-X)

    RIZ  XY (Z=0)  Plane-X = Refsys-X
                   Plane-Y = Refsys-IY
                  (Plane-Z = Refsys-IZ)

    RIY  XZ (Y=0)  Plane-X = Refsys-IX
                   Plane-Y = Refsys-IZ
                  (Plane-Z = Refsys-IY)

    RIX  YZ (X=0)  Plane-X = Refsys-Y
                   Plane-Y = Refsys-IZ
                  (Plane-Z = Refsys-IX)

    ____________________________________________________________________________

    PLN Z-Axis [X-Axis]
    Plane from Z-Axis (normal vector),
      optional origin, X-Axis or point on x-axis, offset along z-axis.

      [Origin]          optional;
      Z-Axis            enter DX or DY or DZ or a vektor;
                        (the Z-axis of the new plane)
      [X-Axis]          optional: the new X-axis; DX or DY or DZ
                        or a defined vector or a point on the new x-axis.
      [offset Z-axis]   optional: distance of the new origin along the
                        new z-axis

    Examples:
    # Plane normal to the Z-axis, with distance.
    R1=PERP DZ 100
    # Plane normal to the Z-axis, through point.
    R2=PERP P(0 0 100) DZ
    # Plane in point p1; normal to the absolute X-axis;
    #   new X-axis direction of absolute Z-axis;
    #   distance 10 into direction of new Z-axis.
    P1=P(100 0 0)
    R3=PERP P1 DX DZ 50

    # Level from origin, normal vector and a point on the x-axis of the new plane
    R11 = PERP P(100 100 100) D(0 0 1) P(101 100 100)

    R12=PERP P(100 150 0) D(ANG(90) ANG(45))

    PLN X-Axis [Y-Axis]
    Plane from X-Axis,
      optional origin, Y-Axis or point on y-axis, offset along z-axis.

      [Origin]          optional;
      X-Axis            Vector or point on the new X-axis
      [Y-Axis]          optional: Vector or point on the new y-axis
      [offset Z-axis]   optional: distance of the new origin along the
                        new z-axis

    Examples:
    # origin, X-axis, Y-axis.
    R12=P(100 100 100) D(1 0 0) D(0 1 0)

    # Level/reference system through three 3D points;
    #  po = the origin,
    #  px = a point on the x-axis of the new plane
    #  pt = a point in the plane (must not be on the line po-px).
    R4 = P(100 100 100) P(101,100,100) P(100,101,100)

    R20=P(100 100 25) DX DY
    R10 = P(100 100 100) DZ
    R11 = P(100 100 100) D(0 0 1) P (101 100 100)
    R13 = P(100 100 100) L(P(0 0 0) P(0 0 100))

    PLN PT Plane Offset Angle
    Move, rotate a plane/reference system
      Set new origin,
      move the origin along X/Y/Z-axis,
      rotate the X-axis and Y-axis around the Z-axis
      All parameters are optional.

      [Origin]         the new orgin
      [Refsys]         plane to be moved
      [offset-X-axis]  move the new origin along the X-axis
      [offset-Y-axis]  move the new origin along the Y-axis
      [offset-Z-axis]  move the new origin along the Z-axis
      [Angle-around-Z] rotate the reference system around Z-axis (degree)

    Example:
    #
    # R20 - set new orgin
    R21=RSYS P(100 100 50) R20
    # R20 - move orgin, rotate axes
    R22=RSYS R20 X(100) Y(100) ANG(180)

    ____________________________________________________________________________
    MAN functions for planes and axis systems (further functions):

    Plane parallel to the XY plane, all axis directions are the same as
      the main axis. The distance on the Z-axis is specified.
      R = Z (Z_distance)
    R5 = Z(100)

    Plane parallel to the YZ plane, and the new X-axis corresponds
      to the 3D Y-axis, the new Y-axis corresponds to the 3D Z-axis.
      The new Z-axis is the axis-X.
      R = X(X_distance)

    Plane parallel to the XZ plane, and the new X-axis corresponds to the
      3D X-axis,
      The new Y-axis corresponds to the 3D Z-axis.
      The new Z-axis is the axis-Y.
      R = Y(Y_distance)

    ____________________________________________________________________________